**Advance Smart GPS & Electromagnetic Brake system**

**ABSTRACT**

Rising incidents of theft vehicles is an increasing concern in cities. The purpose of this project is to eliminate all possibility of theft by using ‘Advance Smart GPS System’. ‘Electromagnetic Brake Systems’ are the future of transportation safety using ‘Eddy Current Law’. Eddy current braking systems are a better alternative to the currently used friction based braking systems for instance disk and drum brakes. Electromagnetic brakes have become a wide regarded, technological advancement, in regards to the reduction of friction and heat energy produced, when braking heavy loads of matter. By Combining ‘Advance Smart GPS’ & ‘Electromagnetic Brake System’ technology can get all the stats of these two system into mobile by creating a Mobile App. These System can be controlled from Mobile app, Smart GPS System is a system in which can integrate all vehicles into one app to track data and analyze from different place regardless of vehicles location. This Smart GPS System Project is copyrighted (©) by ‘Dread Eye Studio’. This project definitively answers the question regarding elimination of theft & future proof. Further studies are needed to establish crucial for safety & preventative measures.

**TABLE OF CONTENTS**

* Acknowledgement
* Abstract
* List of Figures
* List of Tables
* Abbreviation

**Chapter 1: Introduction**

* Introduction and History of Advance Smart GPS System
* Introduction and History of Electromagnetic Brake system

**Chapter 2: Literature Review**

1. Literature Review of Advance Smart GPS System
   1. Active and Passive Tracking System
   2. Type of Tracking System
2. Literature Review of Electromagnetic Brake System
   1. Type of Brake System
   2. Signification/Scopes of Electromagnetic Brake System
   3. Limitations of Electromagnetic Brake System
3. Objectives

**Chapter 3: Hardware Components**

1. Introduction
2. List of Components
   1. DES MC300 Series (model 328)
   2. SIM 908 Module
   3. GPS and GSM antenna
   4. Relay Switch
   5. Battery
   6. Wheel
   7. Frame
   8. Electric Motor

**Chapter 4: Software Components**

1. Introduction
2. List of Services
   1. DES VPS Server
   2. DES Global Map
   3. Database
   4. Mobile App Build
   5. Visual Studio
   6. Arduino IDE

**Chapter 5: Result Analysis \*\*\***

**Chapter 6: Summary and Conclusions**

**References**

**Appendix**

**LIST OF FIGURES**

**LIST OF TABLES**

**ABBREVIATIONS**

DES - Dread Eye Studio

DES MC - Dread Eye Studio Microcontroller

GSM - Global System for Mobile Communication

APN - Access Point Name

GPS - Global System for Mobile Communication

AVL - Automatic Vehicle Location

GIS - Geographic Information System

RF - Radio Frequency

AGPS - Assisted Global Positioning System

RDID - Radio Frequency Identification

DC - Direct Current

AC - Alternating Current

HTTP - Hypertext Transfer Protocol

HTML - Hypertext Markup Language

IDE - Integrated Development Environment

CSS - Cascade Style Sheet

SQL - Structure Query Language

DBMS - Database Management System

JDBC - Java Database connectivity

2D - Two Dimensional

3D - Three Dimensional

XML - Extensible Markup Language

POST - Power On Self Test

EEPROM- Electrically Erasable Programmable Read only Memory

SRAM - Static Random Access Memory

API - Application Programming Interface

**Chapter 1: Introduction**

**1. Introduction and History of Advance Smart GPS System**

The vehicle tracking system is a total security and fleet management solution. It is the technology used to determine the location of a vehicle using different methods like GPS and other navigation system operating via satellite and ground based stations. Modern vehicle tracking system use GPS technology to monitor and locate our vehicle anywhere on earth, but sometimes different types of automatic vehicle location technology are also used. The vehicle tracking system is fitted inside the car that provides effective real time location and the data can even be stored and downloaded to a computer which can be used for analysis in future. This system is an essential device for tracking car any time the owner wants to monitor it and today it is extremely popular among people having expensive cars, used as theft prevention and recovery of the stolen car. The data collected can be viewed on electronic maps via internet and software. The device includes modern hardware and software components that help to track and locate automobiles both online and offline. A tracking system comprises of mainly three parts- vehicle unit, fixed based station and Server (Active System) with software system. The vehicle unit incorporates the hardware part that is the DES MC300 Series (model 328), GPS and GSM modem kept inside the vehicle that is to be tracked. The unit is mainly based on a modem that receives signals from the satellite with the help of GPS antenna. This modem then converts the data and sends the vehicle location information via Internet with mobile application ‘DES navigation GPS’ which is synchronized with the server (DES VPS Server) which can then be send to users mobile. Vehicle Security is a primary concern for all vehicle owners. Owners as well as researchers are always looking for new and upgraded vehicle security systems. For the modernization of technology it is now possible to track and closely monitor vehicle in real time as well as to check the history of vehicles movements. The tracking hardware is installed inside the vehicle in such a manner that it is not visible from outside the vehicle. Hence, it works as a secret unit which continuously sends the coordinates to the monitoring center.

**History:**

Global Positioning Systems (GPS) were designed by the United States Government and military, which the design was intended to be used as surveillance. The GPS was invented as a collaborative effort by the United States Department of Defense and Dr. Ivan Getting as a means to create a satellite course plotting system, primarily used for navigation purposes. At that time, the GPS project cost approximately $12 billion for the design and launch of 18 satellites, six in each of the orbital planes spaced 120 degrees apart, and their ground stations. GPS uses these satellites as reference points to determine and give the accurate geographical positions on map. The idea for a global positioning system was initially planned to be used by military and intelligence organizational during the Cold War, with the introduction of the project stemming from the Soviet-launched spacecraft Sputnik. Since its introduction in the 1960s, GPS has developed into a larger and more advanced satellite network constellation that orbits Earth at fixed points in space to send signals to anyone with a GPS receiver. The signals carry a time code and geographic data point that enables us to display a devices exact position anywhere on the planet. The design of GPS is partly similar to the design of ground-based radio navigation systems, such as LORAN and the Decca Navigator, developed in the early 1940s and were used during World War II. Additional inspiration for the GPS system came when the Soviet Union launched the first Sputnik in 1957. A team of U.S. scientists led by Dr. Richard B. Kershner were monitoring Sputnik's radio transmissions. They discovered that, because of the Doppler Effect, the frequency of the signal being transmitted by Sputnik was higher as the satellite approached and lower as it moves away from them. They realized that since they knew their exact location on the globe, by measuring the Doppler distortion it was possible to pinpoint where the satellite was along its orbit.

**2. Introduction and History of Electromagnetic Brake system**

**Introduction:**

Enhancement in Technology a lot of new technologies are arriving in the braking systems. The principle of braking is depending on the conversion of energy that is converted kinetic energy into thermal energy form of heat. In two wheeler Disc brake and drum brake are used in existing system, both braking are contact type braking as well as the frictional resistance braking. Dude to contact type braking losses are more like the wear and tear and so on. Also maintenance is required more like lubrication, replacement of auxiliary part due to wear and tear. There are few problems in the existing braking system. Realize the importance of the new braking system that reduced common problems mentioned earlier, experiment will be conducted to study of electromagnetic braking system. In this electromagnet electrical supply converted into magnetic field which act as magnetic force on the disc to be braked. In this braking system parameter influence to the braking force which is electrical current, air gap between the disc and the electromagnet etc. These are parameter will be design in this experiment. This type of braking system is more effective than the existing braking system. And all disadvantages of the existing braking system will be minimized in the electromagnetic braking system. Electromagnetic brakes are also called as Electro Mechanical Brakes. Stop motion using electromagnetic force to apply mechanical resistance form of frication. The original name was ‘Electro Mechanical Brakes’ but over the years the name changed to ‘Electromagnetic Brakes’, referring to their actuation method. Since becoming popular in the mid 20th century especially in trains and trams, the variety of application and brakes designs has increased dramatically but the basic operation remains the same. Electromagnetic brakes are the brakes working on the electric power and magnetic power. They work on the principle of electromagnetism. ‘Electromagnetic Brake Systems’ are the future of transportation safety using ‘Eddy Current Law’. Eddy current braking systems are a better alternative to the currently used friction based braking systems for instance disk and drum brakes.

**History:**

It is found that electromagnetic brakes can develop a negative power which represents nearly twice the maximum power output of a typical engine, and at least three times the braking power of an exhaust brake. These performances of electromagnetic brakes make them much more competitive candidate for alternative retardation equipments compared with other retarders. By using the electromagnetic brakes are supplementary retardation equipment, the frictions brakes can be used less frequently and therefore practically never reach high temperatures. The brake linings would last considerably longer before requiring maintenance and the potentially brake fade problem could be avoided. In research conducted by a truck manufacturer, it was proved that the electromagnetic brake assumed 80% of the duty which would otherwise have been demanded of the regular service brake. Furthermore the electromagnetic brake prevents the danger that can arise from the prolonged use of brake beyond their capability to dissipate heat. This is most likely to occur while a vehicle descending a long gradient at high speed. Ina study with a vehicle with 5 axles and weighting 40 tones powered by a powered by an engine of 310 b.h.p travelling down a gradient of 6% at a steady speed between 35 and 40 m.h.p, it can be calculated that the braking power necessary to maintain this speed to the order of 450 hp. The brakes, therefore, would have to absorb 300 hp, meaning that each brake in the 5 axels must absorb 30 hp, that a friction brake can normally absorb with self destruction. The magnetic brake is wall suited to such conditions since it will 9 independently absorb more than 300 hp. It therefore can exceed the requirements of continuous uninterrupted braking, leaving the friction brakes cool and ready for emergency braking in total safety. The installation of an electromagnetic brake is not very difficult if there is enough space between the gearbox and the rear axle. If did not need a subsidiary cooling system. It relay on the efficiency of engine components for its use, so do exhaust and hydrokinetic brakes. The exhaust brake is an on/off device and hydrokinetic brakes have very complex control system. The electromagnetic brake control system is an electric switching system which gives it superior controllability.

**Chapter 2: Literature Review**

**1. Literature Review of Advance Smart GPS System**

Nowadays GPS units are great tracking devices that help fleet managers stay in control of their business. The applications in today’s GPS units make it possible to take full control of any company. It is clear that the tracking devices offer many benefits to companies, since we can build automated expense reports anytime. GPS units do more than just allow companies to create reports. These devices also help to put an end to thieves. According to recent reports, crime is at a high, which means that car theft is increasing. If we have the right GPS unit, we can put an end to car thefts because we can lock and unlock our car anytime we want to. GPS is small tracking device that is installed in a car and it will supply feedback data from tracking software that loads from a satellite. In this paper GPS based vehicle navigation system is implemented. This is done by fetching the information of the vehicle like location, distance, etc. by using GPS and GSM. The information of the vehicle is obtained after every specified time interval defined by the user. Then this periodic information of location is transmitted to monitoring or tracking server. This transmitted information is displayed on the display unit by using the DES Global Map to display the vehicle location in the electronic DES Global Map. This system uses Global Positioning System (GPS) which is used to receive the coordinates of latitude and longitude form the satellite. We all know that tracking system is now a day a very important in modern world. This system can be used in the monitoring our car, also in tracking the theft of the vehicle and in many more other applications. This system uses microcontroller powered by DES MC300 Series (model 328), Global Positioning System (GPS) and Global System for Mobile Communication (GSM). Only one GPS device is used in this system and GSM enable a two way communication process. GSM modem is provide with a SIM card which uses the same and regular communication process as we are using in regular phone. This can also be done with WIFI Interface, If there is existing WIFI available in that source. From the above mentioned vehicle tracking techniques we can say that each technique is appropriate with its function but in some system we need continuous net access and this system can go down if net fails. In the first system the GPS tracks the vehicle location and send it to the controller (DES MC300 Series (model 328)). Its then decide to share via server to the user. On getting the data on user’s side the DES Global Map display the location of the Vehicle on the display unit, this system is useless without net because with ‘Error’ or ‘No Network’ user cont able to receive message sent by controller (DES MC300 Series (model 328)). In this case message is stored/Stack then when connected It send all the information back to that user. By considering all these factors the upcoming implementation should introduce many more facilities which will make the system user friendly and efficient.

**1.1. Active and Passive Tracking System**

Tracking System is classified as ‘passive’ and ‘active’. Passive devices store GPS location, speed, heading and also track information like trigger event for key press, door open or close. Once the vehicle returns to a predetermined point, the device is removed or using WIFI/BLUTOOTH etc to transfer data which then analysis with computer. Were as Active devices also collect same data as passive the only difference is it does in real time via cellular or WIFI over Internet. Passive trackers do not monitor movement in real time. Which mean it monitors it passive in local storage. Which can be accessed which in that source. After we have gathered all of the information we need from a passive tracker, we can place the tracker back on the same (or different) vehicle/source. The main reason people choose passive trackers is that these devices are less expensive than active trackers. GPS passive device are not attached to a monthly fee, which makes there trackers affordable. It all comes down to monitoring vehicle that need to be tracked at regular time interval or Passive way. Were as active GPS tracking devices can access at any time.

**1.2. Type of Tracking System**

There are three main types of GPS vehicle tracking that are widely used. There are:

* Assisted Global Positioning System (AGPS)
* Automatic Vehicle Location (AVL) system
* Radio Frequency Identification (RFID)

**Assisted Global Positioning System (AGPS):**

In AGPS system, a terrestrial RF network is used to improve the performance of GPS receivers as it provides information about the satellite constellation directly to the GPS receivers. AGPS uses both mobiles and cellular networks to locate the accurate positioning information. AGPS is used to overcome limitations of GPS. With unassisted GPS, locating the satellites, receiving the data and confirming the exact position may take several minutes. The tracking method of AGPS uses 4 satellites (3 satellites determine latitude, longitude and elevation and the fourth provides element of time) hence it never fails to detect the location of a vehicle. Location of the vehicle is provided with accuracy of between 3m and 8m, and the speed of 1Km by using this method. Information like vehicle location average speed, direction, and path traversed in a selected period and alerts Engaged/Unengaged, speed limit, vehicle breakdown and traffic jam are delivered by the tracking system to the base station. The system provides continues updates after every 10 seconds while the vehicle is in motion.

**Automatic Vehicle Location (AVL) system:**

In AVL system is an advanced method to track and monitor any remote vehicle with the device that receives and sends signals through GPS satellites. AVL comprises of Global Positioning System (GPS) and Geographic Information System (GIS) in order to provide the real geographic location of the vehicle. AVL system consists of PC-based tracking software to dispatch, a radio system. Among the two types of AVL, GPS based and Signpost based. GPS based system is widely used. The tracking method uses GPS satellite to locate the vehicle equipped with GPS modem by sending satellite signals. The accuracy of the tracking method depends on the AVL system which provides the vehicle location with the accuracy of about 5m to 10m. The information transmitted by the tracking system to the base station is location, speed, direction, mileage, start and stop information and status of vehicle. The information of the vehicle is often transmitted to the central control system (base station) from the vehicle after every 60 seconds. If the base station receives the data, it displays it on a computerized map. GPS receiver on the vehicle receives the signals of its geographic location. Then the receiver sends that data plus speed, direction, etc. to the base station via a radio system. The system also has some limitation using the AVL system we cannot get accurate, complete and sufficient satellite data in dense urban areas or indoors and when transmission is blocked by natural obstructions or many buildings. It can also occur in RF-shadowed environments and under unfriendly Radio Frequency (RF) conditions. Sometimes, a position fix can be impossible.

**Radio Frequency Identification (RFID):**

In RFID is an automatic identification method using devices called tags to store and remotely retrieves data. RFID uses radio waves to capture data from tags. The tracking method of RFID is comprised of three components: tag (passive, semi passive and active), reader (antenna or integrator) and software (middleware). RFID tag which contains microelectronic circuits sends the vehicle information to a remote RFID reader which is then read via the software. This system provides the location of the vehicle with the accuracy of 4m to 6m. Information such as location of the vehicle, mileage and speed are delivered by the tracking system to the centre. The information is updated every one minute. The information is sent to and received from RFID tags by a reader using radio waves.

**2. Literature Review of Electromagnetic Brake System**

**Principle of Electromagnetic Brake System**

If a piece of copper wire wound around the nail bar and then connected to the electrical supply, it would create that substance to act as an electro magnet. The magnetic field that is generated in the wire, from the current is known as “Right Hand Thumb Rule”. The Strength of the magnetic field can be changed by changing both wire size and the amount of wire turns. An Electromagnet is type of temporary magnet in which magnetic field is produced by a flow of electric current. The magnetic fields disappear when the current is lost. The wire produces loops of magnetic field lines around it, the current represents the movement of bar and resulting field line direction is the direction of turning. If a wire is wound into a coil, then the field lines add up in such a way as to produce a set of field lines surround the coil in a similar way to those that surrounds as a permanent bar magnet. If further a piece of soft iron is placed inside the coil, they themselves serve as many little bar magnets in the iron, creating a strong bar magnet as long as the current is switch on.

**Working of Electromagnetic Brake System**

A soft iron core that is magnetized by passing a current through a coil of wire wound on the core. Electromagnets are used to lift heavy masses of magnetic material and to attract movable magnetic parts like iron disc and ferrous material. When electric supply given to the electromagnet then it act as a temporary magnet this magnetic field exerted the force on rotation disc in the direction of perpendicular to the disc. In an engineering sense the word electromagnet does not refer to the electromagnetic brakes and clutches, and in attractive and lifting or holding magnets and magnetic chucks.

Electromagnets may be classified into two types:

* Traction Magnets:

In which the pull is to be exerted over a distance and work is done by reducing the air gap.

* Lifting or holding magnets:

In which the material is initially placed in contact with the magnet For Examples of the latter type are magnetic chucks and circular lifting magnets.

**Design and Practical Working:**

Theoretically, it is divided into three main units are Base unit, Driving unity and Braking Unit. Base unit consist of structural foundation of base unit, driving unit consist of an electrical motor, power control and bearing. Braking unit consists of an electromagnet. Electromagnetic brakes also called as Electro Mechanical Brakes. Stop motion using electromagnetic force to apply mechanical resistance by friction. The original name was “Electro Mechanical Brakes” referring to their actuation method. Since becoming popular in the mid 20th century especially in trains and trolleys, the variety of application and brake current brakes use electromagnetic force but electromagnetic brakes ultimately depend on friction and eddy current brakes use magnetic force directly.

**Material Selection:**

Material Selection process is depending on application of where the brake is used. Generally plate is mostly used in aluminum because it is very efficient to produce eddy current in plate. Preferred to use most effective copper plate but it is not cost efficient.

**2.1. Type of Brake System**

* **Electromagnetic Brake System:**

Rising style of brake system, electromagnetic brakes use an electric motor that is included in the automobile which help the vehicle come to stop. These types of brakes are in most hybrid vehicles and use an electric motor to charge the batteries and regenerative brakes. On occasion some buses will use it as a secondary retarder brake.

* **Frictional Brake System:**

Frictional brake system is found in many automobiles. It is typically found in two forms pads and shoes. As the name implies these brakes use friction to stop the automobile from moving. They typically include a rotating device with a stationary pad and a rotating weather surface. On most band brakes the shoe will constrict and rub against the outside of the rotating drum. Alternatively on a drum brake, a rotating drum with shoes will expand and rub against the inside of the drum.

* **Hydraulic Brake System:**

A hydraulic brake system is composed of a master cylinder that is fed by a reservoir of hydraulic braking fluid. This is connected by an assortment of metal pipes and rubber fittings which are attached to the cylinders of the wheels. The wheels contain two opposite pistons which are located on the band or drum brakes which pressure to push the pistons apart forcing the brake pads into the cylinders, thus causing the wheel to stop moving.

**2.2. Signification/Scopes of Electromagnetic Brake System**

* Electromagnetic brakes satisfy all the energy requirements of braking without the use of friction. They have better heat dissipation capability to avoid problems that friction brakes faces times.
* They can also be used as supplementary retardation equipment in addition to the regular friction brakes on heavy vehicles.
* These brake component cost is less so these brakes are cheap.
* They can be used as an alternative method for the future crisis of the crude oils.

**2.3. Limitations of Electromagnetic Brake System**

* The installation of an electromagnetic brake is very difficult if there is not enough space between the gearbox and rear axle.
* It cannot use grease or oil.
* Electromagnetic brakes are good at slowing things down, not completely stopping them.

**Chapter 3: Hardware Components**

**1. Introduction**

The core function of our project is to develop an electromagnetic brake and GPS tracking system that is cost effective so we have made use of the following hardware components that has effective operation and usage. We made usage of GPS module to capture location, speed and time of last received data in accordance. Then using GSM technology, the captured data already sent to the web server is stored and for this we have used SIM908 module.

**2. List of Components**

The following list of hardware components:

**2.1. DES MC300 Series (model 328)**

Microcontroller which is programmed made as a module is DES MC300 Series (model 328). It is microcontroller board based on the ATmega328PU. It has 32 KB (with 0.5 KB occupied by boot loader). It also has 2 KB of SDRAM and 1 KB of EEPROM (which can be read and written with the EEPROM library). It has 28 pin in total, 20 digital input/output pins of which 6 can be used as PWM output and 6 can be used as analog inputs, in circuit system programming (ICSP). Its clock at 16 MHz continuously no matter what the code is doing.

**2.2. SIM 908 Module**

SIM908 module is a complete Quad-Band GSM / GPRS module which combines GPS technology for satellite navigation. It has a SIM application toolkit where SIM card can be inserted. The compact design which integrated GPRS and GPS in a SMT package significantly saves both time and cost for one to develop GPS enabled applications. A modem GSM & GPRS with SIM908 module allows to create data connections on the GSM network through a standard USB interface. The cellular modems, particularly USB-stick ones, are now at very affordable prices. However, they are limited: they are explicitly designed for Internet connections, so one cannot use it as a normal modem and so implement, for example, a point to point data communications with them.

**2.3. GPS and GSM antenna**

**GPS antenna:**

This GPS antenna draws about 10mA and will give you an additional 28 dB of gain. It got a 5 meter long cable so it will easily reach wherever it is needed to. The antenna is magnetic so it will stick to the top of a car or truck or any other steel structure. GPS signals are extremely weak and present unique demands on the antenna so the choice of antenna plays an important role in GPS performance. A GPS unit needs to have a clear, unobstructed sky view, to best receive the microwave signals that allow it to communicate with satellites. GPS Down/Up converter used for very long cable runs. This GPS antenna that receives the GPS signal, converts it to a lower frequency which is then sent down the cable. Next to the GPS receiver is an up converter that converts the signal back to the original frequency and delivers it to the GPS receiver.

**GSM antenna:**

GSM communications are dependent on antennas. The antenna is what allows communications signals to be sent and received. The antenna that we have used in our project provides operation at both GSM Quad Band Frequencies with +2dBi gain. This antenna operates in Quad Band 890/960, 1710/1880 MHz Frequencies and it’s a unidirectional.

**2.4. Relay Switch**

The electro-mechanical relay is an output device (actuator) which comes in a whole host of shapes, sizes and designs, and has many uses and applications in electronic circuits. But while electrical relays can be used to allow low power electronic or computer type circuits to switch relatively high currents or voltages both ‘ON’ or ‘OFF’, some form of **relay switch circuit** is required to control it. Relay switch is of two types NPN relay switch circuit and PNP relay switch circuit.

**2.5. Battery**

A battery is a device consisting of one or more [electrochemical cells](https://en.wikipedia.org/wiki/Electrochemical_cell) with external connections for powering [electrical](https://en.wikipedia.org/wiki/Electricity) devices such as [flashlights](https://en.wikipedia.org/wiki/Flashlight), [mobile phones](https://en.wikipedia.org/wiki/Mobile_phone), and [electric cars](https://en.wikipedia.org/wiki/Electric_car). When a battery is supplying [electric power](https://en.wikipedia.org/wiki/Electric_power), its positive terminal is the [cathode](https://en.wikipedia.org/wiki/Cathode) and its negative terminal is the [anode](https://en.wikipedia.org/wiki/Anode).

**2.6. Wheel**

**2.7. Frame**

**2.8. Electric Motor**

**Chapter 4: Software Components**

**1. Introduction**

**2. List of Services**

**2.1. DES VPS Server**

**2.2. DES Global Map**

**2.3. Database**

**2.4. Mobile App Build**

**2.5. Visual Studio**

**2.6. Arduino IDE**

**Chapter 5: Result Analysis \*\*\***